


1. Click windows key on keyboard



1. Type “Device Manager”



1. Find Ports (COM & LPT)



1. Remember which COM (e.g. COM20)

A screenshot of a computer error

AI-generated content may be incorrect.

1. Open software DEMO.exe



1. Interface of the software

A screenshot of a computer

AI-generated content may be incorrect.

1. Focus here change

A screenshot of a computer

AI-generated content may be incorrect.

1. Select the COM that you get from Device Manager (eg.COM20)

A screenshot of a computer

AI-generated content may be incorrect.

1. Click Open

A screenshot of a computer

AI-generated content may be incorrect. -> A screen shot of a computer

AI-generated content may be incorrect.

1. Focus here

A screenshot of a computer

AI-generated content may be incorrect.

1. Put your RFID tags on RFID Reader



1. Wait new record coming, copy the text highlighted (**0007ADA9**).

**Same position**

**8 digit number**

**No spacing**

A screenshot of a computer

AI-generated content may be incorrect.

1. **Paste in the system**